=====
SETUP
-1.527
7.927
6.400
main_tx_inst/serializer/channel_cnt_1_s3
2.731
3.190
main_tx_inst/serializer/n285_s6
4.188
4.814
main_tx_inst/serializer/n387_s10
7.269
7.741
main_tx_inst/serializer/n387_s5
7.741
7.918
main_tx_inst/serializer/ch_out_17_s0
7.927
=====
SETUP
-1.468
7.868
6.400
main_tx_inst/serializer/channel_cnt_2_s1
2.731
3.190
main_tx_inst/serializer/n381_s11
4.201
5.300
main_tx_inst/serializer/n382_s13
6.506
7.532
main_tx_inst/serializer/n382_s9
7.532
7.682
main_tx_inst/serializer/n382_s5
7.682
7.859
main_tx_inst/serializer/ch_out_22_s0
7.868
=====
SETUP
-1.458
11.870
10.411
main_rx_1_inst/transmitter/bit_counter_0_s3
2.673
3.132
main_rx_1_inst/transmitter/n1114_s89
5.123
5.749
main_rx_1_inst/transmitter/n1114_s75
5.749
5.898
main_rx_1_inst/transmitter/n1114_s61
5.898
6.061
main_rx_1_inst/transmitter/n1133_s1
7.359
7.985
main_rx_1_inst/transmitter/n1133_s0
8.806
9.432
main_rx_1_inst/transmitter/sdout_1_s0
11.870
=====
SETUP
-1.452
11.863
10.411
main_rx_1_inst/transmitter/bit_counter_0_s3
2.673
3.132
main_rx_1_inst/transmitter/n1102_s55
5.459
6.558
main_rx_1_inst/transmitter/n1102_s53
6.558
6.707
main_rx_1_inst/transmitter/n1102_s49
6.707
6.870
main_rx_1_inst/transmitter/n1135_s2
7.854
8.880
main_rx_1_inst/transmitter/n1135_s0
9.299
9.925
main_rx_1_inst/transmitter/sdout_3_s0
11.863
=====
SETUP
-1.444
7.844
6.400
main_tx_inst/serializer/channel_cnt_1_s3
2.731
3.190
main_tx_inst/serializer/n285_s8
4.188
4.814
main_tx_inst/serializer/n381_s14
6.482
7.508
main_tx_inst/serializer/n381_s13
7.508
7.658
main_tx_inst/serializer/n381_s5
7.658
7.835
main_tx_inst/serializer/ch_out_23_s0
7.844
=====
SETUP
-1.393
7.793
6.400
main_tx_inst/serializer/channel_cnt_2_s1
2.731
3.190
main_tx_inst/serializer/n381_s11
4.201
5.300
main_tx_inst/serializer/n398_s13
6.644
7.466
main_tx_inst/serializer/n398_s9
7.466
7.615
main_tx_inst/serializer/n398_s5
7.615
7.778
main_tx_inst/serializer/ch_out_6_s0
7.793
=====
SETUP
-1.393
7.793
6.400
main_tx_inst/serializer/channel_cnt_2_s1
2.731
3.190
main_tx_inst/serializer/n381_s11
4.201
5.300
main_tx_inst/serializer/n384_s13
6.644
7.466
main_tx_inst/serializer/n384_s9
7.466
7.615
main_tx_inst/serializer/n384_s5
7.615
7.778
main_tx_inst/serializer/ch_out_20_s0
7.793
=====
SETUP
-1.388
7.788
6.400
main_tx_inst/serializer/channel_cnt_1_s3
2.731
3.190
main_tx_inst/serializer/n381_s9
4.188
4.814
main_tx_inst/serializer/n404_s9
7.130
7.602
main_tx_inst/serializer/n404_s5
7.602
7.779
main_tx_inst/serializer/ch_out_0_s0
7.788
=====
SETUP
-1.374
7.774
6.400
main_tx_inst/serializer/channel_cnt_1_s3
2.731
3.190
main_tx_inst/serializer/n381_s9
4.188
4.814
main_tx_inst/serializer/n401_s9
7.116
7.588
main_tx_inst/serializer/n401_s5
7.588
7.765
main_tx_inst/serializer/ch_out_3_s0
7.774
=====
SETUP
-1.369
7.769
6.400
main_tx_inst/serializer/channel_cnt_2_s1
2.731
3.190
main_tx_inst/serializer/n381_s11
4.201
5.300
main_tx_inst/serializer/n400_s13
6.808
7.433
main_tx_inst/serializer/n400_s9
7.433
7.583
main_tx_inst/serializer/n400_s5
7.583
7.760
main_tx_inst/serializer/ch_out_4_s0
7.769
=====
SETUP
-1.369
7.769
6.400
main_tx_inst/serializer/channel_cnt_2_s1
2.731
3.190
main_tx_inst/serializer/n381_s11
4.201
5.300
main_tx_inst/serializer/n392_s13
6.808
7.433
main_tx_inst/serializer/n392_s9
7.433
7.583
main_tx_inst/serializer/n392_s5
7.583
7.760
main_tx_inst/serializer/ch_out_12_s0
7.769
=====
SETUP
-1.360
7.760
6.400
main_tx_inst/serializer/channel_cnt_2_s1
2.731
3.190
main_tx_inst/serializer/n381_s11
4.201
5.300
main_tx_inst/serializer/n395_s13
6.334
7.433
main_tx_inst/serializer/n395_s9
7.433
7.582
main_tx_inst/serializer/n395_s5
7.582
7.745
main_tx_inst/serializer/ch_out_9_s0
7.760
=====
SETUP
-1.300
7.701
6.400
main_tx_inst/serializer/channel_cnt_2_s1
2.731
3.190
main_tx_inst/serializer/n381_s11
4.201
5.300
main_tx_inst/serializer/n383_s13
6.339
7.365
main_tx_inst/serializer/n383_s9
7.365
7.515
main_tx_inst/serializer/n383_s5
7.515
7.692
main_tx_inst/serializer/ch_out_21_s0
7.701
=====
SETUP
-1.249
7.649
6.400
main_tx_inst/serializer/channel_cnt_1_s3
2.731
3.190
main_tx_inst/serializer/n381_s9
4.188
4.814
main_tx_inst/serializer/n403_s9
6.991
7.463
main_tx_inst/serializer/n403_s5
7.463
7.640
main_tx_inst/serializer/ch_out_1_s0
7.649
=====
SETUP
-1.249
7.649
6.400
main_tx_inst/serializer/channel_cnt_1_s3
2.731
3.190
main_tx_inst/serializer/n381_s9
4.188
4.814
main_tx_inst/serializer/n399_s9
6.991
7.463
main_tx_inst/serializer/n399_s5
7.463
7.640
main_tx_inst/serializer/ch_out_5_s0
7.649
=====
SETUP
-1.243
7.643
6.400
main_tx_inst/serializer/channel_cnt_2_s1
2.731
3.190
main_tx_inst/serializer/n381_s11
4.201
5.300
main_tx_inst/serializer/n389_s13
6.494
7.316
main_tx_inst/serializer/n389_s9
7.316
7.465
main_tx_inst/serializer/n389_s5
7.465
7.628
main_tx_inst/serializer/ch_out_15_s0
7.643
=====
SETUP
-1.238
7.639
6.400
main_tx_inst/serializer/channel_cnt_2_s1
2.731
3.190
main_tx_inst/serializer/n381_s11
4.201
5.300
main_tx_inst/serializer/n394_s13
6.678
7.303
main_tx_inst/serializer/n394_s9
7.303
7.453
main_tx_inst/serializer/n394_s5
7.453
7.630
main_tx_inst/serializer/ch_out_10_s0
7.639
=====
SETUP
-1.220
7.621
6.400
main_tx_inst/serializer/channel_cnt_2_s1
2.731
3.190
main_tx_inst/serializer/n381_s11
4.201
5.300
main_tx_inst/serializer/n396_s13
6.660
7.285
main_tx_inst/serializer/n396_s9
7.285
7.435
main_tx_inst/serializer/n396_s5
7.435
7.612
main_tx_inst/serializer/ch_out_8_s0
7.621
=====
SETUP
-1.185
7.585
6.400
main_tx_inst/serializer/channel_cnt_2_s1
2.731
3.190
main_tx_inst/serializer/n381_s11
4.201
5.300
main_tx_inst/serializer/n393_s13
6.159
7.258
main_tx_inst/serializer/n393_s9
7.258
7.407
main_tx_inst/serializer/n393_s5
7.407
7.570
main_tx_inst/serializer/ch_out_11_s0
7.585
=====
SETUP
-1.147
7.547
6.400
main_tx_inst/serializer/channel_cnt_2_s1
2.731
3.190
main_tx_inst/serializer/n333_s5
3.633
4.665
main_tx_inst/serializer/n397_s14
6.185
7.211
main_tx_inst/serializer/n397_s9
7.211
7.361
main_tx_inst/serializer/n397_s5
7.361
7.538
main_tx_inst/serializer/ch_out_7_s0
7.547
=====
SETUP
-1.134
11.546
10.411
main_rx_1_inst/transmitter/bit_counter_0_s3
2.673
3.132
main_rx_1_inst/transmitter/n1120_s80
5.337
5.962
main_rx_1_inst/transmitter/n1120_s71
5.962
6.112
main_rx_1_inst/transmitter/n1120_s69
6.112
6.289
main_rx_1_inst/transmitter/n1120_s65
6.289
6.466
main_rx_1_inst/transmitter/n1134_s2
6.891
7.990
main_rx_1_inst/transmitter/n1134_s0
8.811
9.437
main_rx_1_inst/transmitter/sdout_2_s0
11.546
=====
SETUP
-1.083
7.483
6.400
main_tx_inst/serializer/channel_cnt_2_s1
2.731
3.190
main_tx_inst/serializer/n381_s11
4.201
5.300
main_tx_inst/serializer/n386_s13
6.334
7.156
main_tx_inst/serializer/n386_s9
7.156
7.305
main_tx_inst/serializer/n386_s5
7.305
7.468
main_tx_inst/serializer/ch_out_18_s0
7.483
=====
SETUP
-1.060
7.460
6.400
main_tx_inst/serializer/channel_cnt_1_s3
2.731
3.190
main_tx_inst/serializer/n381_s9
4.188
4.814
main_tx_inst/serializer/n390_s9
6.802
7.274
main_tx_inst/serializer/n390_s5
7.274
7.451
main_tx_inst/serializer/ch_out_14_s0
7.460
=====
SETUP
-1.060
7.460
6.400
main_tx_inst/serializer/channel_cnt_1_s3
2.731
3.190
main_tx_inst/serializer/n381_s9
4.188
4.814
main_tx_inst/serializer/n385_s9
6.802
7.274
main_tx_inst/serializer/n385_s5
7.274
7.451
main_tx_inst/serializer/ch_out_19_s0
7.460
=====
SETUP
-1.044
7.771
6.727
i2s_in_sclk_ibuf
0.000
2.088
main_tx_inst/clocks/i2s_lrclk_s2
2.332
2.790
main_tx_inst/deserializer/n2035_s0
3.949
4.751
main_tx_inst/deserializer/sample_ch_4_l_buf_0_s0
7.771
=====
HOLD
0.142
2.844
2.702
i2s_in_sclk_ibuf
0.000
1.392
main_tx_inst/clocks/aes_lrclk_s2
1.577
1.910
main_tx_inst/serializer/zaes_lrck_s0
2.844
=====
HOLD
0.558
1.254
0.696
main_rx_1_inst/clocks/bsync_pos_edge_s0
0.683
1.016
main_rx_1_inst/clocks/i2s_bclk_s2
1.254
=====
HOLD
0.561
3.187
2.626
main_rx_1_inst/deserializer/bsync_pos_edge_s0
2.614
2.947
main_rx_1_inst/deserializer/channel_counter_0_s0
3.187
=====
HOLD
0.565
3.191
2.626
main_rx_1_inst/clocks/zzaes_lrclk_s0
2.614
2.947
main_rx_1_inst/clocks/aes_lrclk_pos_edge_s0
3.191
=====
HOLD
0.568
3.195
2.626
main_rx_1_inst/receiver/aes3_clk_s0
2.614
2.947
main_rx_1_inst/receiver/sync_cnt_4_s0
3.195
=====
HOLD
0.587
1.283
0.696
main_rx_1_inst/clocks/zzbsync_s0
0.683
1.016
main_rx_1_inst/clocks/bsync_pos_edge_s0
1.283
=====
HOLD
0.594
3.221
2.626
main_rx_1_inst/receiver/aes3_clk_s0
2.614
2.947
main_rx_1_inst/receiver/sync_cnt_2_s0
3.221
=====
HOLD
0.594
3.221
2.626
main_rx_1_inst/receiver/aes3_clk_s0
2.614
2.947
main_rx_1_inst/receiver/sync_cnt_3_s0
3.221
=====
HOLD
0.671
3.373
2.702
i2s_in_sclk_ibuf
0.000
1.392
main_tx_inst/clocks/i2s_bclk_s2
1.577
1.910
main_tx_inst/deserializer/zbclk_s0
3.373
=====
HOLD
0.708
3.380
2.672
main_tx_inst/deserializer/lrck_neg_edge_s4
2.672
3.005
main_tx_inst/deserializer/n30_s2
3.008
3.380
main_tx_inst/deserializer/lrck_neg_edge_s4
3.380
=====
HOLD
0.708
3.322
2.614
main_rx_1_inst/transmitter/bit_counter_1_s3
2.614
2.947
main_rx_1_inst/transmitter/n30_s3
2.950
3.322
main_rx_1_inst/transmitter/bit_counter_1_s3
3.322
=====
HOLD
0.708
3.322
2.614
main_rx_1_inst/transmitter/bclk_neg_edge_s4
2.614
2.947
main_rx_1_inst/transmitter/n8_s2
2.950
3.322
main_rx_1_inst/transmitter/bclk_neg_edge_s4
3.322
=====
HOLD
0.708
3.322
2.614
main_rx_1_inst/clocks/count_i2s_lrclk_7_s0
2.614
2.947
main_rx_1_inst/clocks/n229_s2
2.950
3.322
main_rx_1_inst/clocks/count_i2s_lrclk_7_s0
3.322
=====
HOLD
0.708
3.322
2.614
main_rx_1_inst/clocks/count_i2s_lrclk_30_s0
2.614
2.947
main_rx_1_inst/clocks/n206_s2
2.950
3.322
main_rx_1_inst/clocks/count_i2s_lrclk_30_s0
3.322
=====
HOLD
0.708
3.322
2.614
main_rx_1_inst/receiver/reg_clk_period_0_s0
2.614
2.947
main_rx_1_inst/receiver/n79_s2
2.950
3.322
main_rx_1_inst/receiver/reg_clk_period_0_s0
3.322
=====
HOLD
0.708
3.322
2.614
main_rx_1_inst/receiver/sync_cnt_5_s0
2.614
2.947
main_rx_1_inst/receiver/n22_s2
2.950
3.322
main_rx_1_inst/receiver/sync_cnt_5_s0
3.322
=====
HOLD
0.708
2.284
1.577
i2s_in_sclk_ibuf
0.000
1.392
main_tx_inst2/transmitter/data_biphase_s1
1.577
1.910
main_tx_inst2/transmitter/n2535_s2
1.912
2.284
main_tx_inst2/transmitter/data_biphase_s1
2.284
=====
HOLD
0.708
2.284
1.577
i2s_in_sclk_ibuf
0.000
1.392
main_tx_inst/clocks/aes_lrclk_s2
1.577
1.910
main_tx_inst/clocks/n264_s3
1.912
2.284
main_tx_inst/clocks/aes_lrclk_s2
2.284
=====
HOLD
0.708
2.284
1.577
i2s_in_sclk_ibuf
0.000
1.392
main_tx_inst/clocks/count_aes_lrclk_0_s0
1.577
1.910
main_tx_inst/clocks/n255_s2
1.912
2.284
main_tx_inst/clocks/count_aes_lrclk_0_s0
2.284
=====
HOLD
0.708
2.284
1.577
i2s_in_sclk_ibuf
0.000
1.392
main_tx_inst/clocks/count_i2s_lrclk_0_s0
1.577
1.910
main_tx_inst/clocks/n143_s2
1.912
2.284
main_tx_inst/clocks/count_i2s_lrclk_0_s0
2.284
=====
HOLD
0.708
1.391
0.683
main_rx_1_inst/clocks/count_i2s_bclk_0_s0
0.683
1.016
main_rx_1_inst/clocks/n62_s2
1.019
1.391
main_rx_1_inst/clocks/count_i2s_bclk_0_s0
1.391
=====
HOLD
0.709
2.285
1.577
i2s_in_sclk_ibuf
0.000
1.392
main_tx_inst2/transmitter/frame_counter_0_s0
1.577
1.910
main_tx_inst2/transmitter/n95_s2
1.913
2.285
main_tx_inst2/transmitter/frame_counter_0_s0
2.285
=====
HOLD
0.709
2.285
1.577
i2s_in_sclk_ibuf
0.000
1.392
main_tx_inst/transmitter/data_biphase_s1
1.577
1.910
main_tx_inst/transmitter/n2535_s2
1.913
2.285
main_tx_inst/transmitter/data_biphase_s1
2.285
=====
HOLD
0.709
2.285
1.577
i2s_in_sclk_ibuf
0.000
1.392
main_tx_inst/transmitter/frame_counter_0_s0
1.577
1.910
main_tx_inst/transmitter/n95_s2
1.913
2.285
main_tx_inst/transmitter/frame_counter_0_s0
2.285
=====
HOLD
0.709
2.285
1.577
i2s_in_sclk_ibuf
0.000
1.392
main_tx_inst/transmitter/bit_counter_0_s0
1.577
1.910
main_tx_inst2/transmitter/n10_s2
1.913
2.285
main_tx_inst/transmitter/bit_counter_0_s0
2.285
